DI | VFX FOR MODERN INDEPENDENT FILM PRODUCTION
Dailies and Editorial Proxy Specification
Preserves source identity, timebase, framing, sync, viewing, and relink through editorial.
How to use: Accept or replace each recommended value. Complete the amber column, issue the document to the named recipients, and retain the approved revision.
Document control
	Field or test
	Recommended default or requirement
	Production value or result

	Show
	Full project title and short production code
	

	Spec ID
	PROJECT-DAILIES-SPEC
	

	Revision
	v001. Increment for every issued change.
	

	Issued
	ISO date and time with time zone
	

	Effective
	Immediately unless a future handoff is named
	

	Supersedes
	None for the first issue. Otherwise, name the prior revision.
	

	Prepared by
	Named person, role, company, and contact
	

	Approved by
	Named production and technical approvers
	

	Issued to
	Named people and companies
	

	Acknowledgment record
	Recipient, date, revision received, and exceptions
	

	Authoritative location
	One production-controlled file or record
	



Specification
	Field or test
	Recommended default or requirement
	Production value or result

	Editorial application and project
	[no default - must be specified]
	

	Proxy codec and wrapper
	ProRes Proxy QuickTime for most small productions. Use DNxHR LB MXF when the Avid workflow requires it.
	

	Proxy raster
	1920x1080 with the approved active image and framing
	

	Proxy frame rate
	Match the project timebase exactly
	

	Timecode
	Preserve source timecode and reel or camera-roll identity. Record any duplicate-timecode exception.
	

	Camera metadata
	Preserve source clip name, camera roll, lens data, exposure index, white balance, and source rate where available
	

	Sound sync
	Sync 48 kHz production audio and retain source audio timecode, file name, track names, and channel mapping
	

	Color processing
	Apply the approved camera input, final dailies CDL, Show LUT or creative transform, and viewing transform
	

	Color tags
	Rec.709 review media tagged with NCLC values 1-1-1
	

	Burn-ins
	Project, source clip, source timecode, record timecode, camera roll, and framing reference
	

	Editorial metadata delivery
	[no default - must be specified] Use ALE, XML, or the NLE-native record required by editorial.
	

	Proxy naming
	Preserve the source clip name or maintain a tested one-to-one relink table
	

	Delivery and retention
	[no default - must be specified] Record the production-controlled location and vendor deletion date.
	



Verification
	Field or test
	Recommended default or requirement
	Production value or result

	Relink
	Relink at least one clip from proxy to camera original with zero-frame timing error
	

	Sync
	Check first and last synchronized frames of each production day
	

	Image path
	Compare the proxy against the approved dailies view on the named display
	

	Evidence
	Test clip IDs, result, reviewer, date, and exceptions
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