DI | VFX FOR MODERN INDEPENDENT FILM PRODUCTION
Review-Media Specification
Defines a review proxy, its frame correspondence, and the decisions it can support.
How to use: Accept or replace each recommended value. Complete the amber column, issue the document to the named recipients, and retain the approved revision.
Document control
	Field or test
	Recommended default or requirement
	Production value or result

	Show
	Full project title and short production code
	

	Spec ID
	PROJECT-REVIEW-MEDIA-SPEC
	

	Revision
	v001. Increment for every issued change.
	

	Issued
	ISO date and time with time zone
	

	Effective
	Immediately unless a future handoff is named
	

	Supersedes
	None for the first issue. Otherwise, name the prior revision.
	

	Prepared by
	Named person, role, company, and contact
	

	Approved by
	Named production and technical approvers
	

	Issued to
	Named people and companies
	

	Acknowledgment record
	Recipient, date, revision received, and exceptions
	

	Authoritative location
	One production-controlled file or record
	



Specification
	Field or test
	Recommended default or requirement
	Production value or result

	Codec and wrapper
	H.264 QuickTime
	

	Raster
	1920x1080 with the approved framing
	

	Frame rate
	Match the project timebase
	

	Quality floor
	20 Mb/s for 1920x1080 H.264. Increase the rate for a larger raster, high frame rate, grain, or difficult motion. Inspect the exact file before review.
	

	Review-platform proxy
	A review service may create a lower-quality streaming proxy. Inspect the streamed image. When compression affects a note, check the uploaded source or a full-quality still before assigning work.
	

	Color encoding
	Rec.709 / BT.1886
	

	Color tags
	Write nclc or nclx values equivalent to 1-1-1 for Rec.709 review media, as supported by the wrapper.
	

	Viewing transform
	Same named creative and viewing chain used for approved production review
	

	Framing
	Match the current editorial framing, with letterbox or pillarbox included where required
	

	Handles
	Show the cut range in editorial context. Include handles only for a named technical review.
	

	Burn-ins
	Project, shot ID, revision, state, frame, record timecode, vendor, and date
	

	Start timecode
	01:00:00:00 for every review QuickTime unless another value is agreed before vendor onboarding
	

	Audio
	Current stereo editorial reference at 48 kHz
	

	Review platform
	Frame.io for most independent productions, with password and recipient controls
	

	Approval authority
	Named person and scope of approval
	

	Permitted decisions
	VFX creative and timing review. Final color and image-quality approval require the named calibrated display.
	

	Retention
	Export approvals and notes before the platform's deletion or account-closure date
	



Correspondence test
	Field or test
	Recommended default or requirement
	Production value or result

	QuickTime-to-EXR correspondence
	Record test shot, QuickTime start and end, EXR range, and DI verification
	

	Color comparison
	Compare the QuickTime and final EXR through the same viewing transform
	

	Evidence
	Test IDs, reviewer, date, result, and exceptions
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