DI | VFX FOR MODERN INDEPENDENT FILM PRODUCTION
Asset and Delivery Manifest Specification
Defines the file-level inventory and integrity record for a delivery.
How to use: Accept or replace each recommended value. Complete the amber column, issue the document to the named recipients, and retain the approved revision.
Document control
	Field or test
	Recommended default or requirement
	Production value or result

	Show
	Full project title and short production code
	

	Spec ID
	PROJECT-MANIFEST-SPEC
	

	Revision
	v001. Increment for every issued change.
	

	Issued
	ISO date and time with time zone
	

	Effective
	Immediately unless a future handoff is named
	

	Supersedes
	None for the first issue. Otherwise, name the prior revision.
	

	Prepared by
	Named person, role, company, and contact
	

	Approved by
	Named production and technical approvers
	

	Issued to
	Named people and companies
	

	Acknowledgment record
	Recipient, date, revision received, and exceptions
	

	Authoritative location
	One production-controlled file or record
	



Specification
	Field or test
	Recommended default or requirement
	Production value or result

	Production asset ID
	Stable ID assigned by production
	

	Identifier scope
	Production asset register or named authority
	

	Recipient asset ID
	Record when assigned. Do not replace the production ID.
	

	Revision
	v###
	

	Source vendor revision
	Record separately when supplied
	

	Variant
	Original, textless, localized, censored, alternate, or another named purpose
	

	Representation
	Format, raster, color encoding, language, or another technical form
	

	State
	Use only the controlled vocabulary on this page
	

	Asset class and purpose
	Picture master, VFX final, audio stem, timed text, project, or another named class
	

	Filename or relative path
	One row per file for integrity verification
	

	Byte size
	Exact integer for each file
	

	Checksum and algorithm
	SHA-256 by default. Use the recipient's required method when supplied.
	

	File-set manifest
	Per-file hashes or MHL for an image sequence or package
	

	Derived from
	Source asset ID and revision
	

	Source timing
	Source clip and timecode or source frame range
	

	Record timing
	Timeline timecode or delivery frame range
	

	Language and territory
	BCP 47 language tag and named territory where applicable
	

	Technical properties
	Picture, audio, timed-text, project, or package properties required to interpret the file
	

	Package or composition ID
	Package ID, CPL UUID, or Not applicable
	

	Creator and creation date
	Person or vendor and ISO date and time
	

	Change reason
	Concise description of the change
	

	Approver and approval date
	Named person and ISO date and time
	

	Delivered to and sent date
	Named recipient, delivery ID, and date
	

	Received by and received date
	Named recipient contact and date
	

	Acceptance state
	Accepted, rejected, or accepted with listed exceptions
	

	Storage location
	Production-controlled copy location after delivery
	

	Access classification
	Public, production, confidential, restricted, or another defined class
	

	Retention
	Deletion or migration date and responsible custodian
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